IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "Project Number"
Time stamp: "2020-01-29T17:23:44"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20180806_1515(x64) - Exporter 19.1.0.112 - Alternate UI 19.1.0.112"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "info@bimetica.com" of Organization (no name given)
  Owner history of Person "info@bimetica.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1580314752 (2020-01-29T16:19:12Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "1Â½H x 1Â½H" | object type "1Â½H x 1Â½H" | names: "2019_Valvula_Arco_Tajo:1Â½H x 1Â½H:281347" | material: materials ("Jatón Europeo CW617N - Chromado", "Color Negro") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Graphics, Identity Data

Types
  IFCVALVETYPE "1Â½H x 1Â½H" | 1 occurrence | material: materials ("Jatón Europeo CW617N - Chromado", "Color Negro") | property sets: Construction, Data, Dimensions, General, Green Building Properties, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Pipe Accessories" (IFCLABEL)
    Family = "2019_Valvula_Arco_Tajo: 1Â½H x 1Â½H" (IFCLABEL)
    Family and Type = "2019_Valvula_Arco_Tajo: 1Â½H x 1Â½H" (IFCLABEL)
    Type = "2019_Valvula_Arco_Tajo: 1Â½H x 1Â½H" (IFCLABEL)
    Type Id = "2019_Valvula_Arco_Tajo: 1Â½H x 1Â½H" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Story Level" (IFCLABEL)
    Family and Type = "Level: Story Level" (IFCLABEL)
    Type = "Level: Story Level" (IFCLABEL)
    Type Id = "Level: Story Level" (IFCLABEL)
  Other | properties | on 1 type object
    Ancho Símbolo = 0.0492490387104011 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Category = "Pipe Accessories" (IFCLABEL)
    CondicionesEvaluacion = 0. (IFCREAL)
    Contacto = "" (IFCTEXT)
    ContenidoGarantia = "" (IFCTEXT)
    CosteMantenimiento = 0. (IFCREAL)
    DescripcionEvaluacion = 0. (IFCREAL)
    Exclusiones = "" (IFCTEXT)
    Family Name = "2019_Valvula_Arco_Tajo" (IFCTEXT)
    FechaEvaluacion = 0. (IFCREAL)
    FechaFinGarantia = "" (IFCTEXT)
    FechaInicioGarantia = "" (IFCTEXT)
    GarantiaExtendida = TRUE (IFCBOOLEAN)
    HEX = TRUE (IFCBOOLEAN)
    IdentificadorGarantia = "" (IFCTEXT)
    Mantenimiento = "" (IFCTEXT)
    OCT = FALSE (IFCBOOLEAN)
    PeriodoGarantia = "" (IFCTEXT)
    PuntoDeContacto = "" (IFCTEXT)
    TiempoMedioEntreFallos = "" (IFCTEXT)
    TiempoUtilDeVida = "" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Story Level" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Grid Line 1/2"" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Level Head - Circle: Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    AnoProduccion = "" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Autor = "Bimetica PDS" (IFCTEXT)
    BIM Support = "https://bimsupport.info/es/fabricantes/valvulas-arco-bim/" (IFCTEXT)
    BasePrecioProducto01 = "" (IFCTEXT)
    BasePrecioProducto02 = "" (IFCTEXT)
    BasePrecioProducto03 = "" (IFCTEXT)
    Bimetica = "www.bimetica.com" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Codigo = "00009" (IFCTEXT)
    CondicionesDeVenta = "" (IFCTEXT)
    Cost = 5.8 (IFCREAL)
    Description = "Válvula Tajo mando palanca H-H" (IFCTEXT)
    EmailContacto = "info@valvulasarco.es" (IFCTEXT)
    EtiquetaModelo = "Arco_Tajo" (IFCTEXT)
    FechaEmisionElementoBIM = "30/01/2020" (IFCTEXT)
    FechaVencimientoElementoBIM = "30/01/2021" (IFCTEXT)
    Historial = "(RVT2019-V01) Creación del elemento" (IFCTEXT)
    InformacionTecnica = "" (IFCTEXT)
    Manufacturer = "Vávulas Arco S.L" (IFCTEXT)
    Marcado CE = TRUE (IFCBOOLEAN)
    Model = "Tajo" (IFCTEXT)
    Numero de Declaracion de Prestaciones = "" (IFCTEXT)
    Numero de Licencia = "XXX-XXXX9536" (IFCTEXT)
    NumeroArticulo = "" (IFCTEXT)
    NumeroArticuloGlobalComercial = "" (IFCTEXT)
    OmniClass Number = "23.65.55.14.21" (IFCTEXT)
    OmniClass Title = "Non-Return Valves for Liquid Services" (IFCTEXT)
    PaisVenta = "España y Portugal" (IFCTEXT)
    PartidaURL = "" (IFCTEXT)
    Referencia = "00009" (IFCTEXT)
    ReferenciaContactoComercialVenta = "" (IFCTEXT)
    ReferenciaContactoSoporteTecnico = "" (IFCTEXT)
    Serie = "Tajo" (IFCTEXT)
    TelefonoContacto = "0034 963 17 10 70" (IFCTEXT)
    Titular = "Vávulas Arco S.L" (IFCTEXT)
    Type Comments = "Agua potable, agua caliente sanitaria y aire comprimido" (IFCTEXT)
    Type Name = "1Â½H x 1Â½H" (IFCTEXT)
    URL = "www.valvulasarco.com" (IFCTEXT)
    URL de Declaracion de Prestaciones = "" (IFCTEXT)
    URLPerfilProductoBimetica = "https://bimetica.com/es/valvula-tajo-3235.html" (IFCTEXT)
    URLProducto = "" (IFCTEXT)
    UnidadMedicion = "" (IFCTEXT)
    Version = "RVT2019" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Vávulas Arco S.L" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "2019_Valvula_Arco_Tajo:1Â½H x 1Â½H" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Maximum Size = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Minimum Size = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Size = "2"ø-2"ø" (IFCTEXT)
    Volume = 0.0128363021347507 (IFCVOLUMEMEASURE) [CUBIC FOOT (conversion based)]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Dimensions | properties | on 1 type object
    A = 0.354330708661417 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    B = 0.498687664041995 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    C = 0.351049868766404 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    D = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Diámetro Nominal = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    E = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radio Cuerpo 2 = 0.00328083989501312 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radio Cuerpo = 0.052 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radio Exterior = 0.08 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radio Nominal = 0.0625 (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Radio Tuerca = 0.08 (IFCLENGTHMEASURE) [FOOT (conversion based)]
  Graphics | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Insulation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [FOOT (conversion based)]
    Overall Size = "2"ø-2"ø" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    K Coefficient = 113.2 (IFCREAL)
  Mechanical - Flow | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Pressure Drop = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "Project Completion" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Construction | properties | on 1 type object
    Espacio = "" (IFCTEXT)
    ResponsablePrescripcion = "" (IFCTEXT)
    Sistema = "Agua potable, agua caliente sanitaria y aire comprimido" (IFCTEXT)
    Zona = "" (IFCTEXT)
  Data | properties | on 1 type object
    CurvaSonido = 0. (IFCREAL)
  General | properties | on 1 type object
    CodigoBarras = "" (IFCTEXT)
    FechaColocacion = "" (IFCTEXT)
    FechaCompra = "" (IFCTEXT)
    FechaSuministro = "" (IFCTEXT)
    InstruccionesEspeciales = "" (IFCTEXT)
    LugarEnsamblaje = "" (IFCTEXT)
    MaterialContenedor = "" (IFCTEXT)
    MaterialEnvoltura = "" (IFCTEXT)
    NumeroSerie = "" (IFCTEXT)
    ReferenciaLote = "" (IFCTEXT)
    ResponsableCompra = "" (IFCTEXT)
    TipoEmbalajeProteccion = "" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    AcidificacionAtmosfericaPorUnidad = 0. (IFCREAL)
    AguaConsumidaPorUnidad = 0. (IFCREAL)
    CambioClimaticoPorUnidad = 0. (IFCREAL)
    Creditos BREEAM = "" (IFCTEXT)
    Creditos LEED = "" (IFCTEXT)
    DestruccionCapaOzonoEstratosfericaPorUnidad = 0. (IFCREAL)
    Energia consumida = 0. (IFCREAL)
    EnergiaNoRenovableConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaPrimariaTotalConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaRenovableConsumidaPorUnidad = 0. (IFCREAL)
    EutrofizacionPorUnidad = 0. (IFCREAL)
    FaltaDeRecursosPorUnidad = 0. (IFCREAL)
    FaseCicloVida = "" (IFCTEXT)
    FormacionFotoquimicaOzonoPorUnidad = 0. (IFCREAL)
    ResiduoInertePorUnidad = 0. (IFCREAL)
    ResiduoRadioactivoPorUnidad = 0. (IFCREAL)
    ResiduosNoPeligrososPorUnidad = 0. (IFCREAL)
    ResiduosPeligrososPorUnidad = 0. (IFCREAL)
    Unidad = "" (IFCTEXT)
    VidaUtilEsperada = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Acabado = "Cromado" (IFCTEXT)
    MaterialCarcasa = "Jatón Europeo CW617N - Chromado" (IFCLABEL)
  Segments and Fittings | properties | on 1 type object
    ClasificacionDeCierre = 0. (IFCPRESSUREMEASURE) [PASCAL]
    CoeficienteDeCaudal = 113.2 (IFCREAL)
    MecanismoValvula = "BALL" (IFCTEXT)
    OperacionValvula = "PALANCA" (IFCTEXT)
    PatronValvula = "STRAIGHT_2_PORT" (IFCTEXT)
    PresionDePrueba = 0. (IFCPRESSUREMEASURE) [PASCAL]
    PresionDeTrabajo = 0. (IFCPRESSUREMEASURE) [PASCAL]
    Tamano = 0.125 (IFCLENGTHMEASURE) [FOOT (conversion based)]