IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
File name: "Projektnummer"
Time stamp: "2017-02-22T11:30:28"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)"

People and organizations
  Person "Mklein" of Organization (no name given)
  Owner history of Person "Mklein" of Organization (no name given) | application "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 48° 8′ 20.852966″ | longitude 11° 34′ 48.669204″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Projektadresse", "München", "Deutschland"
      IFCBUILDINGSTOREY "Ebene 0" | long name "Ebene 0" | elevation 0.
        contains 3 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "infraSchwank D 80 LL" | names: "Heater-Schwank_GmbH-Tube_Heaters-infraSchwank_LL__02-2017:infraSchwank D 80 LL:332064" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Low Gloss - Black", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic- Schwank - Smooth") | property sets: Phasen, Sonstige, HLS, Abhängigkeiten, ID-Daten, Elektro - Lasten
          1 x IFCBUILDINGELEMENTPROXY | object type "infraSchwank D 100 LL" | names: "Heater-Schwank_GmbH-Tube_Heaters-infraSchwank_LL__02-2017:infraSchwank D 100 LL:332085" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Low Gloss - Black", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic- Schwank - Smooth") | property sets: Phasen, Abhängigkeiten, HLS, Elektro - Lasten, Sonstige, Abmessungen
          1 x IFCBUILDINGELEMENTPROXY | object type "infraSchwank D 120 LL" | names: "Heater-Schwank_GmbH-Tube_Heaters-infraSchwank_LL__02-2017:infraSchwank D 120 LL:332106" | material: materials ("Paint - Schwank - Flaked Reflective - Beige", "Plastic - Schwank - Low Gloss - Black", "Plastic - Schwank - Coarse Textured - Dark Gray", "Plastic- Schwank - Smooth") | property sets: Materialien und Oberflächen, HLS-Volumenstrom, Text, Abhängigkeiten, Sonstige, Abmessungen

Property sets
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 0" (IFCTEXT)
    Bottom Clearance to Combustibles = 1.7 (IFCLENGTHMEASURE) [METRE]
    Burner Side Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Ebene = "Ebene: Ebene 0" (IFCLABEL)
    Flue Gas Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Top Clearance to Combustibles = 0.25 (IFCLENGTHMEASURE) [METRE]
    Versatz = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 0" (IFCTEXT)
    Bottom Clearance to Combustibles = 2.3 (IFCLENGTHMEASURE) [METRE]
    Burner Side Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Ebene = "Ebene: Ebene 0" (IFCLABEL)
    Flue Gas Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Top Clearance to Combustibles = 0.35 (IFCLENGTHMEASURE) [METRE]
    Versatz = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Front Clearance to Combustibles = 0.45 (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 0" (IFCTEXT)
    Bottom Clearance to Combustibles = 3. (IFCLENGTHMEASURE) [METRE]
    Burner Side Clearance to Combustibles = 0.2 (IFCLENGTHMEASURE) [METRE]
    Ebene = "Ebene: Ebene 0" (IFCLABEL)
    Flue Gas Clearance to Combustibles = 0.15 (IFCLENGTHMEASURE) [METRE]
    Top Clearance to Combustibles = 0.45 (IFCLENGTHMEASURE) [METRE]
    Versatz = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Front Clearance to Combustibles = 0.25 (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Front Clearance to Combustibles = 0.35 (IFCLENGTHMEASURE) [METRE]
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 16711680 (IFCINTEGER)
    Linienmuster = "Verdeckt" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol = "Beschriftung Ebene: Beschriftung Ebene" (IFCLABEL)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)
  Materialien und Oberflächen | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Heater = "Matal - Schwank - Copper - Satin Brushed" (IFCLABEL)
    Pipe Material = "Plastic - Schwank - Coarse Textured - Dark Gray" (IFCLABEL)
    Unit = "Paint - Schwank - Flaked Reflective - Beige" (IFCLABEL)
  HLS-Volumenstrom | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Airflow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasen | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Phase 1" (IFCLABEL)
  Sonstige | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Angle Control = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Edit Formula Control = TRUE (IFCBOOLEAN)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle Control = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Edit Formula Control = FALSE (IFCBOOLEAN)
  Sonstige | properties | on 1 object (1 IFCBUILDING)
    Kundenname = "Bauherr" (IFCTEXT)
    Projektadresse = "Projektadresse" (IFCTEXT)
    Projektausgabedatum = "Projekt Datum" (IFCTEXT)
    Projektname = "Projektname" (IFCTEXT)
    Projektnummer = "Projektnummer" (IFCTEXT)
    Projektstatus = "Projektstatus" (IFCTEXT)
    Verfasser Firma 1 = "Firma 1" (IFCTEXT)
    Verfasser Firma 2 = "Firma 2" (IFCTEXT)
    Verfasser PLZ Ort = "PLZ Ort" (IFCTEXT)
    Verfasser Strasse = "Strasse" (IFCTEXT)
    Verfasser Telefax = "Telefax" (IFCTEXT)
    Verfasser Telefon = "Telefon" (IFCTEXT)
    Verfasser eMail = "E-Mail" (IFCTEXT)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Dimension A = 0.25 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 1.7 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.5 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.7 (IFCLENGTHMEASURE) [METRE]
    Dimension H = 0.15 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Dimension A = 0.35 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 2.3 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.7 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 2.3 (IFCLENGTHMEASURE) [METRE]
    Dimension H = 0.15 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Dimension A = 0.45 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.2 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 3. (IFCLENGTHMEASURE) [METRE]
    Dimension D = 0.15 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 1. (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.2 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 3. (IFCLENGTHMEASURE) [METRE]
    Dimension H = 0.15 (IFCLENGTHMEASURE) [METRE]
  HLS | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Gas Pressure Line Minimum = 457.2 (IFCREAL)
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Systemklassifizierung = "Sonstige,Energie,Sonstige,Energie,Abluft 2" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Pressure Line Minimum = 609.6 (IFCREAL)
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Systemklassifizierung = "Sonstige,Energie,Sonstige,Energie,Abluft 2" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Inlet Radius = 0.00953 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line Maximum = 1828.8 (IFCREAL)
    IR Output = 59500. (IFCPOWERMEASURE) [WATT]
    Radiant Efficiency = "59.1%" (IFCTEXT)
    Rating Natural Gas = 78000. (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = "94%" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Inlet Radius = 0.00953 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line Maximum = 1828.8 (IFCREAL)
    IR Output = 74800. (IFCPOWERMEASURE) [WATT]
    Radiant Efficiency = "60.2%" (IFCTEXT)
    Rating Natural Gas = 98000. (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = "94%" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Flow Rate = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Inlet Radius = 0.00953 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line Maximum = 1828.8 (IFCREAL)
    IR Output = 91600. (IFCPOWERMEASURE) [WATT]
    Radiant Efficiency = "59.4%" (IFCTEXT)
    Rating Natural Gas = 120000. (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = "94%" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "1" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "2" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "3" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 0" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDING)
    Autor = "" (IFCTEXT)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "Tube Heater, infraSchwank D 80 LL" (IFCTEXT)
    Cost Info = "" (IFCTEXT)
    Hersteller = "Schwank GmbH" (IFCTEXT)
    Manufacturer Address = "Bremerhavener Str. 43, D-50733 Köln" (IFCTEXT)
    Manufacturer Email = "mailto:info@schwank.de" (IFCTEXT)
    Manufacturer Fax = "49-221-7176-288" (IFCTEXT)
    Manufacturer Phone = "49-221-7176-0" (IFCTEXT)
    Modell = "infraSchwank D 80 LL" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Line = "infraSchwank" (IFCTEXT)
    Product Page URL = "" (IFCTEXT)
    Subcategory = "Tube Heaters" (IFCTEXT)
    URL = "www.schwank.de" (IFCTEXT)
    Weight = 5308.69830708661 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "Tube Heater, infraSchwank D 100 LL" (IFCTEXT)
    Cost Info = "" (IFCTEXT)
    Hersteller = "Schwank GmbH" (IFCTEXT)
    Manufacturer Address = "Bremerhavener Str. 43, D-50733 Köln" (IFCTEXT)
    Manufacturer Email = "mailto:info@schwank.de" (IFCTEXT)
    Manufacturer Fax = "49-221-7176-288" (IFCTEXT)
    Manufacturer Phone = "49-221-7176-0" (IFCTEXT)
    Modell = "infraSchwank D 100 LL" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Line = "infraSchwank" (IFCTEXT)
    Product Page URL = "" (IFCTEXT)
    Subcategory = "Tube Heaters" (IFCTEXT)
    URL = "www.schwank.de" (IFCTEXT)
    Weight = 7239.13405511811 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "Tube Heater, infraSchwank D 120 LL" (IFCTEXT)
    Cost Info = "" (IFCTEXT)
    Hersteller = "Schwank GmbH" (IFCTEXT)
    Manufacturer Address = "Bremerhavener Str. 43, D-50733 Köln" (IFCTEXT)
    Manufacturer Email = "mailto:info@schwank.de" (IFCTEXT)
    Manufacturer Fax = "49-221-7176-288" (IFCTEXT)
    Manufacturer Phone = "49-221-7176-0" (IFCTEXT)
    Modell = "infraSchwank D 120 LL" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Line = "infraSchwank" (IFCTEXT)
    Product Page URL = "" (IFCTEXT)
    Subcategory = "Tube Heaters" (IFCTEXT)
    URL = "www.schwank.de" (IFCTEXT)
    Weight = 7882.61263779528 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  Elektro - Lasten | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Element = "" (IFCTEXT)
    Stromkreisnummer = "" (IFCTEXT)
  Elektro - Lasten | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Apparent Load = 0. (IFCREAL)
    Load Classification = "Other" (IFCLABEL)
    Load Sub Classification Motor = FALSE (IFCBOOLEAN)
    Power Factor = 1. (IFCREAL)
  Abmessungen | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Minimum Mounting Height = 5.5 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.445 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 14.065 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Left = 0.05 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Right = 0.13 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.47 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 18.94 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Left = 0.05 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Right = 0.13 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Exhaust Radius = 0.05 (IFCLENGTHMEASURE) [METRE]
    Heater Box Length = 0.47 (IFCLENGTHMEASURE) [METRE]
    Height = 0.315 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 20.04 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Left = 0.05 (IFCLENGTHMEASURE) [METRE]
    Pipe Offset Right = 0.13 (IFCLENGTHMEASURE) [METRE]
    Width = 0.584 (IFCLENGTHMEASURE) [METRE]
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Schwank GmbH" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "infraSchwank D 80 LL" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "infraSchwank D 100 LL" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "infraSchwank D 120 LL" (IFCIDENTIFIER)
  Text | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Brochure URL = "" (IFCTEXT)
    Manual URL = "" (IFCTEXT)
    Technical Information = "" (IFCTEXT)
    Warranty URL = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Eigenschaften für ökologisches Bauen | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    ecoScorecard Product Page = "http://ecoscorecard.com/" (IFCTEXT)
  Konstruktion | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Exhaust Air Connector = "Exhaust Air Connector" (IFCTEXT)
    Gas Inlet Connector = "Gas Inlet Connection" (IFCTEXT)
    Power Connector = "Power Connection" (IFCTEXT)
  Elektro | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Electrical Supply Amperage = 0. (IFCREAL)
    Electrical Supply Frequency = 50. (IFCREAL)
    Electrical Supply Voltage = 2475.69939584324 (IFCREAL)
    Number of Poles = 1 (IFCINTEGER)