IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
File name: "Projektnummer"
Time stamp: "2017-02-22T12:43:42"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)"

People and organizations
  Person "Mklein" of Organization (no name given)
  Owner history of Person "Mklein" of Organization (no name given) | application "Autodesk Revit 2014 (DEU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (DEU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 48° 8′ 20.852966″ | longitude 11° 34′ 48.669204″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Projektadresse", "München", "Deutschland"
      IFCBUILDINGSTOREY "Ebene 0" | long name "Ebene 0" | elevation 0.
        contains 4 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "SupraSchwank-10" | names: "Space_Heater-Schwank-High_Intensity-supraSchwank:SupraSchwank-10:330319" | material: materials ("Matal - Schwank - Semi - Polished", "Matal - Schwank - Copper - Satin Brushed") | property sets: Abhängigkeiten, Elektro - Lasten, Phasen, ID-Daten, Abmessungen, HLS
          1 x IFCBUILDINGELEMENTPROXY | object type "SupraSchwank-15" | names: "Space_Heater-Schwank-High_Intensity-supraSchwank:SupraSchwank-15:330329" | material: materials ("Matal - Schwank - Semi - Polished", "Matal - Schwank - Copper - Satin Brushed") | property sets: HLS, Abhängigkeiten, Abmessungen, Elektro - Lasten, Phasen, Sonstige
          1 x IFCBUILDINGELEMENTPROXY | object type "SupraSchwank-20" | names: "Space_Heater-Schwank-High_Intensity-supraSchwank:SupraSchwank-20:330339" | material: materials ("Matal - Schwank - Semi - Polished", "Matal - Schwank - Copper - Satin Brushed") | property sets: Elektro - Lasten, ID-Daten, Abhängigkeiten, HLS, Sonstige, Abmessungen
          1 x IFCBUILDINGELEMENTPROXY | object type "SupraSchwank-30" | names: "Space_Heater-Schwank-High_Intensity-supraSchwank:SupraSchwank-30:330352" | material: materials ("Matal - Schwank - Semi - Polished", "Matal - Schwank - Copper - Satin Brushed") | property sets: Eigenschaften für ökologisches Bauen, Elektro - Lasten, Konstruktion, Sonstige, Elektro, Abhängigkeiten

Property sets
  Abhängigkeiten | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Basisbauteil = "Ebene : Ebene 0" (IFCTEXT)
    Bottom Clearance to Combustibles = "Dimension G" (IFCTEXT)
    Ebene = "Ebene: Ebene 0" (IFCLABEL)
    Front Clearance to Combustibles = "Dimension D" (IFCTEXT)
    Rear Clearance to Combustibles = "Dimension F" (IFCTEXT)
    Top Clearance to Combustibles = "Dimension E" (IFCTEXT)
    Versatz = 0. (IFCLENGTHMEASURE) [METRE]
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Basishöhe = "Projekt-Basispunkt" (IFCIDENTIFIER)
  Abhängigkeiten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Ansicht = 0. (IFCLENGTHMEASURE) [METRE]
  Grafiken | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Farbe = 16711680 (IFCINTEGER)
    Linienmuster = "Verdeckt" (IFCLABEL)
    Linienstärke = "1" (IFCIDENTIFIER)
    Symbol = "Beschriftung Ebene: Beschriftung Ebene" (IFCLABEL)
    Symbol bei Ende 1 Standard = FALSE (IFCBOOLEAN)
    Symbol bei Ende 2 Standard = TRUE (IFCBOOLEAN)
  Eigenschaften für ökologisches Bauen | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    ecoScorecard Product Page = "http://ecoscorecard.com/" (IFCTEXT)
  Elektro - Lasten | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Apparent Load = 0. (IFCREAL)
    Load Classification = "Power" (IFCLABEL)
    Load Sub Classification Motor = FALSE (IFCBOOLEAN)
    Number of Poles = 1 (IFCINTEGER)
    Power Factor = 1. (IFCREAL)
    Voltage = 0. (IFCREAL)
  Elektro - Lasten | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Element = "" (IFCTEXT)
    Stromkreisnummer = "" (IFCTEXT)
  Phasen | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Phase erstellt = "Phase 1" (IFCLABEL)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "1" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "2" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "3" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Kennzeichen = "4" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Gebäudegeschoss = TRUE (IFCBOOLEAN)
    Name = "Ebene 0" (IFCTEXT)
    Tragwerk = FALSE (IFCBOOLEAN)
  ID-Daten | properties | on 1 object (1 IFCBUILDING)
    Autor = "" (IFCTEXT)
    Beschreibung von Unternehmen = "" (IFCTEXT)
    Gebäudename = "" (IFCTEXT)
    Unternehmensname = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "High Intensity Heaters, supraSchwank – 10" (IFCTEXT)
    Cost Info = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Hersteller = "Schwank" (IFCTEXT)
    Manufacturer Address = "2 Schwank Way, Waynesboro, GA 30830" (IFCTEXT)
    Manufacturer Email = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Manufacturer Fax = "1-866-724-9265" (IFCTEXT)
    Manufacturer Phone - Toll Free = "1-877-446-3727" (IFCTEXT)
    Manufacturer Phone = "1-877-446-3727" (IFCTEXT)
    Modell = "SupraSchwank- 10" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Page URL = "http://www.schwankusa.com/high-intensity-heaters/supra/" (IFCTEXT)
    Subcategory = "High Intensity Heaters" (IFCTEXT)
    URL = "http://www.schwankusa.com" (IFCTEXT)
    Weight = 539.974408676635 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  ID-Daten | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    04 CSI = "23 83 33" (IFCTEXT)
    95 CSI = "15768" (IFCTEXT)
    Baugruppenbeschreibung = "Heat Generating Systems" (IFCTEXT)
    Baugruppenkennzeichen = "D3020" (IFCTEXT)
    Beschreibung = "High Intensity Heaters, supraSchwank - 15" (IFCTEXT)
    Cost Info = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Hersteller = "Schwank" (IFCTEXT)
    Manufacturer Address = "2 Schwank Way, Waynesboro, GA 30830" (IFCTEXT)
    Manufacturer Email = "mailto:csr@schwankgroup.com" (IFCTEXT)
    Manufacturer Fax = "1-866-724-9265" (IFCTEXT)
    Manufacturer Phone - Toll Free = "1-877-446-3727" (IFCTEXT)
    Manufacturer Phone = "1-877-446-3727" (IFCTEXT)
    Modell = "SupraSchwank- 15" (IFCTEXT)
    OmniClass-Nummer = "23.75.10.17.14.14" (IFCTEXT)
    OmniClass-Titel = "Fuel-Fired Radiant Heaters" (IFCTEXT)
    Product Page URL = "http://www.schwankusa.com/high-intensity-heaters/supra/" (IFCTEXT)
    Subcategory = "High Intensity Heaters" (IFCTEXT)
    URL = "http://www.schwankusa.com" (IFCTEXT)
    Weight = 773.476855671937 (IFCREAL)
    ecoScorecard_data = "" (IFCTEXT)
  ID-Daten: 2 more contents on 2 objects not shown
  Abmessungen | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Höhe für Berechnung = 0. (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Heater Box Length = 0.606298 (IFCLENGTHMEASURE) [METRE]
    Height = 0.295275 (IFCLENGTHMEASURE) [METRE]
    Minimum Mounting Height = 4.572 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 0.860298 (IFCLENGTHMEASURE) [METRE]
    Width = 0.508 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Heater Box Length = 0.87884 (IFCLENGTHMEASURE) [METRE]
    Height = 0.295275 (IFCLENGTHMEASURE) [METRE]
    Minimum Mounting Height = 5.4864 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 1.13284 (IFCLENGTHMEASURE) [METRE]
    Width = 0.508 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Heater Box Length = 1.16205 (IFCLENGTHMEASURE) [METRE]
    Height = 0.295275 (IFCLENGTHMEASURE) [METRE]
    Minimum Mounting Height = 6.096 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 1.41605 (IFCLENGTHMEASURE) [METRE]
    Width = 0.508 (IFCLENGTHMEASURE) [METRE]
  Abmessungen | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Heater Box Length = 1.7145 (IFCLENGTHMEASURE) [METRE]
    Height = 0.295275 (IFCLENGTHMEASURE) [METRE]
    Minimum Mounting Height = 7.3152 (IFCLENGTHMEASURE) [METRE]
    Overall Length with Controls = 1.9685 (IFCLENGTHMEASURE) [METRE]
    Width = 0.508 (IFCLENGTHMEASURE) [METRE]
  HLS | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Systemklassifizierung = "Energie,Sonstige" (IFCTEXT)
    Systemname = "" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Radius = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line WC Maximum = "14" (IFCTEXT)
    Gas Pressure Line WC Minimum = "6" (IFCTEXT)
    Gas Pressure WC Manifold = "5" (IFCTEXT)
    IR Output = 6682.02039992667 (IFCPOWERMEASURE) [WATT]
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Radiant Efficiency = "77.2%" (IFCTEXT)
    Rating Natural Gas = 8645.59657008056 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = ">85%" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Radius = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line WC Maximum = "14" (IFCTEXT)
    Gas Pressure Line WC Minimum = "6" (IFCTEXT)
    Gas Pressure WC Manifold = "5" (IFCTEXT)
    IR Output = 10149.0511600641 (IFCPOWERMEASURE) [WATT]
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Radiant Efficiency = "78.7%" (IFCTEXT)
    Rating Natural Gas = 12895.1270875778 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = ">85%" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Radius = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line WC Maximum = "14" (IFCTEXT)
    Gas Pressure Line WC Minimum = "6" (IFCTEXT)
    Gas Pressure WC Manifold = "5" (IFCTEXT)
    IR Output = 13695.2111091479 (IFCPOWERMEASURE) [WATT]
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Radiant Efficiency = "79.2%" (IFCTEXT)
    Rating Natural Gas = 17291.1931401611 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = ">85%" (IFCTEXT)
  HLS | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Radius = 0.00635 (IFCLENGTHMEASURE) [METRE]
    Gas Pressure Line WC Maximum = "14" (IFCTEXT)
    Gas Pressure Line WC Minimum = "6" (IFCTEXT)
    Gas Pressure WC Manifold = "5" (IFCTEXT)
    IR Output = 21013.1957313483 (IFCPOWERMEASURE) [WATT]
    Liquid Propane = FALSE (IFCBOOLEAN)
    Natural Gas = TRUE (IFCBOOLEAN)
    Radiant Efficiency = "81.1%" (IFCTEXT)
    Rating Natural Gas = 25936.7897102417 (IFCPOWERMEASURE) [WATT]
    Thermal Efficiency = ">85%" (IFCTEXT)
  Sonstige | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Angle Control = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Box Width C = 1.70307 (IFCLENGTHMEASURE) [METRE]
    Dimension A = 0.4064 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.9144 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 2.54 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 1.8288 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.6096 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.2032 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.8288 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDING)
    Kundenname = "Bauherr" (IFCTEXT)
    Projektadresse = "Projektadresse" (IFCTEXT)
    Projektausgabedatum = "Projekt Datum" (IFCTEXT)
    Projektname = "Projektname" (IFCTEXT)
    Projektnummer = "Projektnummer" (IFCTEXT)
    Projektstatus = "Projektstatus" (IFCTEXT)
    Verfasser Firma 1 = "Firma 1" (IFCTEXT)
    Verfasser Firma 2 = "Firma 2" (IFCTEXT)
    Verfasser PLZ Ort = "PLZ Ort" (IFCTEXT)
    Verfasser Strasse = "Strasse" (IFCTEXT)
    Verfasser Telefax = "Telefax" (IFCTEXT)
    Verfasser Telefon = "Telefon" (IFCTEXT)
    Verfasser eMail = "E-Mail" (IFCTEXT)
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Box Width C = 0.594868 (IFCLENGTHMEASURE) [METRE]
    Dimension A = 0.4064 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.762 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 2.286 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 1.6764 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.6096 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.2032 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.6764 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Box Width C = 0.86741 (IFCLENGTHMEASURE) [METRE]
    Dimension A = 0.4064 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.762 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 2.4384 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 1.6764 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.6096 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.2032 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.6764 (IFCLENGTHMEASURE) [METRE]
  Sonstige | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Base = FALSE (IFCBOOLEAN)
    Box Width C = 1.15062 (IFCLENGTHMEASURE) [METRE]
    Dimension A = 0.4064 (IFCLENGTHMEASURE) [METRE]
    Dimension B = 0.8382 (IFCLENGTHMEASURE) [METRE]
    Dimension C = 2.54 (IFCLENGTHMEASURE) [METRE]
    Dimension D = 1.7526 (IFCLENGTHMEASURE) [METRE]
    Dimension E = 0.6096 (IFCLENGTHMEASURE) [METRE]
    Dimension F = 0.2032 (IFCLENGTHMEASURE) [METRE]
    Dimension G = 1.7526 (IFCLENGTHMEASURE) [METRE]
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Schwank" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "SupraSchwank-10" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "SupraSchwank-15" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "SupraSchwank-20" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "SupraSchwank-30" (IFCIDENTIFIER)
  Konstruktion | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Gas Inlet Connector = "Gas Inlet Connector" (IFCTEXT)
    Power Connector = "Power Connection" (IFCTEXT)
  Elektro | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Control Amperage = 0.55 (IFCREAL)
    Control Frequency = 60. (IFCREAL)
    Control Voltage = 258.333850001033 (IFCREAL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Text | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Brochure URL = "http://www.schwankusa.com/fileadmin/pdf/Schwank%20Literature/Product_Brochures/supraSchwank%20October%2024.pdf" (IFCTEXT)
    Manual URL = "http://www.schwankusa.com/fileadmin/pdf/Manuals/High_Intensity_Heaters/supra_primo_Manual_12C_NOV-2011.pdf" (IFCTEXT)
    Technical Information = "http://www.schwankusa.com/fileadmin/pdf/Manuals/High_Intensity_Heaters/supra_primo_Manual_12C_NOV-2011.pdf" (IFCTEXT)
    Warranty URL = "http://www.schwankusa.com/fileadmin/pdf/Forms/Schwank_Warranty_Summary_Nov-2012.pdf" (IFCTEXT)
  Materialien und Oberflächen | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Heater = "Matal - Schwank - Copper - Satin Brushed" (IFCLABEL)
    Unit = "Matal - Schwank - Semi - Polished" (IFCLABEL)